WILL-O HOMES CONSTRUCTION SPECIFICATION SHEET ---ARISS
1. Architecturally controlled community designed homes with genuine clay brick,
structural precast stone, Hardie Board (or equivalent) siding and trim, decorative
moldings and accent features.* House siting and exterior colour packages will be
architecturally controlled.
2. Architectural features including detailed dormers, metal roofs, decorative brackets, decorative columns, finials, shutters, turrets, box bay windows and copulas, as per elevation.
3. Corner lot elevations to receive enhanced details, as per Architectural Control.
4. 2' x 6' exterior stud walls with sheathing.**
5. Engineered roof systems with raised heel trusses.
6. Prefinished aluminum soffits, fascia, frieze, eaves troughs and downspouts, as per
elevation.
7. Premium architectural shingles.
8. Pre-finished seamed metal roofs, as per elevation.*
9. Wood and steel beam construction.
10. 3/4" premium engineered OSB tongue & groove subfloor, nailed, glued & screwed.**
11. 7/16" OSB roof sheathing.
12. Engineered floor joist system for all subfloors, not including landings.
13. Poured concrete basement walls with heavy duty damp proofing, weeping tiles, and
exterior drainage membrane.
14. Poured concrete porch at main entrance. 
15. 9’ ceiling height on main floor, 9' ceiling on 2nd floor(as per plan), loft areas(as per plan), except where bulkheads and/or dropped ceilings apply.**
16. Optional door from garage to exterior, grade permitting.*
17. Concrete garage floor 
18. Rough-in BBQ gas line to rear of home NOT included in base price
19. Three piece rough-in plumbing in basement.*
20. Two car garage or three car garage, storage areas, as per plan.
21. Garage interior to be finished with drywall, one coat of tape for fume proofing.
22. PEX (cross-linked polyethylene) hot and cold-water lines throughout.
23. Front cold cellar with vent.
24. Sump pump where applicable.*

DOORS & WINDOWS
1. Premium 8' high insulated main front entry systems, featuring stained wood-grain texture with sidelight(s) and/or transom(s).* Grip set(s) with deadbolt lock on front elevation doors.* - as per elevation plan
2. All exterior doors, windows and building perforations to be foam insulated and fully caulked.
3. Insulated metal door from garage into house 
4. Thermopane Energy Star® qualified coloured vinyl casement windows on all front,
side, and rear elevations. Coloured window frames as per the exterior colour packages
approved by the Controlling Architect.  Standard basement windows to be Energy Star® qualified white vinyl sliders. All windows, including basement windows, to be double-glazed with low emissive coating, argon filled gas with insulated edge spacer bars for greater energy cost savings. All operable windows have screens. Some decorative windows are fixed glass.
5. Extra-large basement windows, 24" high**. Window wells to be installed to accommodate standard basement window(s) depending on grade, at Vendor’s discretion.
6. Extra tall windows to all main floor side and rear windows.*
7. Purchaser’s choice of door styles, smooth finish, decorative-panel interior
passage & closet doors throughout, from Vendor’s standard samples.*
8. Vendor’s choice of pewter finish or brushed satin nickel finish levers and hinges
(hinges not painted) throughout.

ELECTRICAL
1. Twenty (20) interior pot lights on main floor ceiling.  All pot lights are energy efficient with LED bulbs. Locations selected by Purchaser(s) and approved by Vendor.
2. EV charger rough-in, location determined by vendor.
3. 200 AMP service with circuit breakers and copper wiring throughout.
4. Heavy-duty cable and outlet for oven and dryer, plus outlet for gas range only.
5. Electrical outlet for washing machine in laundry room.
6. Exterior GFI protected electrical outlets. One (1) at the front main entrance, one (1)
at the rear door. 
7. Electrical outlets in garage: one (1) per car park on the wall and two (2) outlets in garage ceiling for future installation of garage door opener(s) at Vendor’s sole discretion. Garage door opener(s) not supplied.*
8. Deleted
9. Ceiling fixtures in foyer, hallways, laundry room, breakfast room, kitchen, servery,
mudroom, walk-in pantry, media room, office, sitting room, loft, recreation room and
all bedrooms to have Energy Star® LED light bulbs. Vendor supplied fixtures.*
10. Capped ceiling outlets: one (1) in the dining room, one (1) in the living room, one (1)
in the great room, one (1) in the loft, (1) in the office and (1) in the library room, with a
switch provided for future light fixtures.*
11. All electrical switches and outlets to be white Décora.
12. Prewired for television (RG6 cable) and telephone (CAT5e cable) in great room,
kitchen, media room, office, loft, recreation room, rear loggia and all bedrooms.*
13. Front door entry chimes, as per plan.
14. Electronic smoke detectors on all levels of the home and carbon monoxide detectors
on all levels that have bedrooms as per code
15. All plugs to be protected with arc fault breaker(s) as per code.
16. Rough-in central vacuum outlets centrally located on each finished level in
finished areas. Pipes dropped to unfinished space in basement only.
17. Dedicated electrical outlet for refrigerator and dishwasher.
18. Electrical outlet provided below counter within kitchen island and/or peninsula
cabinet, as per code (only applicable on the island when the island is permanently
fixed with plumbing).*

HEATING & INSULATION
1. Upgraded R31 expandable spray foam insulation to garage ceiling and exterior
overhangs where there are livable areas above.
2. Exterior walls above grade insulated to R22. R50 blown insulation in all attic space
above living areas.
3. Basement walls full height with R20 blanket insulation to approximately 6” above the
basement slab.
4. High-efficiency, 95% efficient, 2 stage forced air gas furnace including central air conditioning. Location and orientation may vary at Vendor’s discretion without notice.*
5. High efficiency condensing gas fired hot water heater on a rental basis with designated
supplier at Vendor’s sole discretion.  The buyer agrees to enter into a rental contract with the supplier selected by the vendor
6. All homes to be equipped with an ERV (Energy Recovery Ventilator) paired with the furnace. Only one ERV supplied per home.
7. Electronic programmable thermostat(s), centrally located on the main floor. Location
of thermostat(s) at Vendor’s discretion.
8. All supply and return metal ductwork joints throughout the home are sealed for better
delivery of conditioned air. 

LAUNDRY ROOM & MUD ROOM
1. “Oatey” box (or equivalent) recessed in the wall in the vicinity of the washer to
facilitate ease of connection of washing machine hot and cold-water lines as well
as the drain.
2. Single stainless steel basin laundry tub where shown on plan to have two (2) handle
faucet and to be set in a base cabinet.
3. Laundry uppers, in white melamine only, over washer and dryer.*(where applicable)
4. Base cabinets in laundry and mudroom, as per plan, to be white melamine with choice
of laminate top from Vendor’s standard samples.

INTERIOR DETAILS
1. Interior walls to be painted with two (2) coats of warm grey premium quality latex
paint; one (1) coat prime plus one (1) finish coat. One colour throughout.
2. All interior doors and trim to be painted with two (2) coats of white premium quality
semi-gloss finish; one (1) primer plus one (1) finish. Hinges not painted.
3. Smooth ceilings throughout. **
4. Interior doors to be 8' high on main floor, 6'-8" on second floor.*(as per plan)
5. Main staircase  to be stained oak veneer, in Purchaser’s choice of colour from Vendor’s
standard samples.*
6. Oak handrails and nosing** stained in choice of colour from Vendor’s
standard samples.  Wrought iron spindles from builder samples
7. Trim with 5-1/4" Modern style baseboards** and 3" Modern style casing**
throughout all finished areas.
8. Privacy locks on primary bedroom and all bathroom doors.

KITCHEN & SERVERY FEATURES
1. Upgraded kitchen & servery cabinetry to have a wide range of door styles and colours
available for Purchaser(s) to choose from Vendor’s standard samples.
2. Kitchen base cabinetry to include one (1) set of bank of drawers, one (1) 2-drawer pot
& pan drawers and colour-matched kick plates.* Purchaser’s choice from Vendor’s
standard samples.
3. All kitchen cabinet drawers and doors to include ‘soft close’ hinge hardware.
4. Extended upper cabinets in the kitchen and servery.*
5. Granite and Quartz counter tops in kitchen and servery to have standard profile edge and clean cut back.* Purchaser’s choice of colour and material from Vendor’s standard samples.
6. Island in kitchen to have flush extended breakfast counter.* Cabinet interiors to be
finished in white melamine.
7. Full depth fridge gables with deep upper cabinet above fridge.*
8. Double stainless steel undermount sink with upgraded single lever pullout spray faucet in kitchen.
9. Single stainless steel undermount sink in servery with single lever faucet.*
10. White vinyl coated wire shelving for the kitchen walk-in pantry.* Maximum three (3) shelves.(where applicable as per plan)
11. Dropped ceiling boxes over kitchen cabinets as required, at Vendor’s discretion.

PRIMARY, POWDER ROOM & SECONDARY BATHROOMS
1. Cabinetry for all bathrooms to have a wide range of door styles and colours available
for Purchaser(s) to select from Vendor’s standard samples.
2. Powder room and formal powder room to have upgraded base cabinet with marble or
quartz countertop, upgraded faucet and undermount sink from Vendor’s standard samples.*
3. Primary ensuite, powder room and formal powder room to have upgraded elongated
energy efficient water saver toilet.
4. Primary ensuite, powder room and formal powder room to have upgraded two handle water efficient vanity faucet(s) 
5. Primary ensuite to have a rectangular free standing acrylic tub with built-in two handle
tub mounted faucet.* as per plan
6. Primary ensuite vanity(ies) to have a bank of drawers or bottom drawer; Vendor’s choice.* Vanities with single sink to have top drawer. As per plan
7. Primary ensuite to have marble or quartz countertop with standard profile edge,
Purchaser(s) choice from Vendor’s standard samples.
8. Primary ensuite sink(s) to be rectangular undermount.*
9. All secondary bathrooms to have marble or quartz counter tops, Purchaser’s choice
from Vendor’s standard sample, with undermount sink(s).
10. Mirrors in all bathrooms. Wall mounted lighting fixture(s) above mirror in all
bathrooms. One mirror and light per sink.*
11. Single lever water efficient faucets in all bathroom vanities.
12. Energy efficient water saver showerhead and toilets.
13. Exhaust fan in all bathrooms.
14. Bathroom accessory package to include toilet paper dispenser and towel bar,
in chrome finish. 
15. DensShield® tile backer with built-in moisture barrier in shower stall and tub enclosures.
16. Bathroom fixtures to be white.

FLOORING FEATURES
1. 6" x 3/4" pre-finished, stained oak strip hardwood flooring** throughout, excluding tiled areas. Purchaser’s choice of stained hardwood from Vendor’s standard samples.
2. 12" x 24" ceramic/porcelain tile in tiled areas on main floor and primary ensuite 
as per plan*.  Flooring allowance as per agreement

EXTERIOR FEATURES
1. Vendor’s choice of address plaque with municipal number at front of home.
2. Lights at front door, garage doors, rear loggia and side doors, as per plan.
3. Two (2) exterior water taps with inside shut-off valves. One (1) located in garage and
one (1) located at the back of the house, location at Vendor’s sole discretion.
4. Front and side of lot to be fully sodded except driveway and landscaped areas,
balance of lot to be seeded.
5. Sectional roll-up garage doors pre-finished metal or metal clad exterior, Vendor’s choice, with heavy-duty springs, decorative inserts and rust resistant door hardware, as per elevation.
6. Driveway to have gravel base
7. Where “lookout basement” (LOB) conditions or “walk out basement” (WOB)
conditions exist, the location of windows and stairs will vary, as per Vendor’s
Architect’s recommendations.
VENDOR’S GUARANTEE
1. All selections, including upgrades, are to be made from Vendor’s samples.
2. Will-O Homes (C.S) Inc is registered with Tarion Warranty Corporation. Tarion
coverage: One (1) year warranty on defects in workmanship and materials. Two (2) year
warranty on electrical, plumbing and heating delivery and distribution system, water
penetration through building envelope and foundation. Seven (7) year warranty on major
structural defects. Purchaser agrees to pay Tarion enrolment fee on closing date.
3. Will-O Homes (C.S) Inc is licensed with the Home Construction Regulatory Authority, the HCRA.
4. The Purchaser acknowledges that they have been advised of and do hereby agree to all
of the following, specific and general notices, warnings, cautions and limitations as
are set out below. Provided that specific terms shall not in any way diminish or replace
general terms of the same or similar nature or kind.
*Availability determined by house design and or grades.
**All measurements, specifications, sizes and finishing details are approximate and
subject to change without notice.
5. In accordance with the Agreement of Purchase and Sale, the Vendor shall have the
right to substitute other products and materials for those listed in this Schedule or
provided for in the plans and specifications provided that the substituted products and
materials are of a quality equal to, or better than, the products and materials so listed
or so provided.
6. Vendor’s samples are subject to natural variations in colour and grain. Floor and wall
tiles, all countertops, laminate flooring, kitchen cabinets, vanity cabinets and wall
finishes are subject to pattern, shade and colour variations.
7. Carpet: The Berber and/or Sisal carpet installed in the home at the Property will not
be a seamless installation. The carpet seams will be visible and accepted as installed
by the Vendor or the Vendor’s agent. Any such seams shall not be considered an item
which is damaged or incomplete for the purposes of the Purchaser’s Pre-Delivery
Inspection and for the completion of the Purchaser’s Pre-Delivery Inspection Form.
8. Deleted
9. Tile: The nature of the rectangular tiles (eg. 12" x 24", etc.) are inherently curved
and uneven. Once installed in the home, especially in a brick pattern style, they
will accentuate the unevenness and bowed appearance in the centre of the tile. Any
inconsistency of the installation of irregular size tiles will not be a warrantable item under Tarion Construction Performance Guidelines. Unevenness shall not be considered an item which is damaged or incomplete for the purpose of the Purchaser’s Pre-Delivery
Inspection and completion of the Purchaser’s Pre-Delivery Inspection Form.
10. Smooth ceilings: Due to the factory finish of gypsum drywall panels and the
conventional methods of concealing joints and fasteners with the products available
today, certain conditions may detract from the quality of the “smooth” finish of the
ceilings. Even though the gypsum drywall panel surface is meticulously treated and
as smooth as possible, conditions involving a combination of lighting (both natural
and electrical) and gloss-enamel or high-gloss paint may bring about shadows which
accentuate even the slightest surface variation across the face of the panel. These surface
variations in colour and sheen may affect the quality of the finished product and in all
likelihood will be most visible where there are treated joints, fastener heads, or corner
beads. To eliminate the problems noted above, the recommended installation is that your
ceiling surfaces be finished with a machine-applied medium to heavy texture spray.
11. Stained stairs: The hardwood flooring to be installed is factory finished through an
automated process, whereas the stained Staircase will be finished manually on-site. As
well, the materials used by the contractors assembling the Staircase do not use material
from the same suppliers and as such, the stain will not be absorbed in the same fashion
for each piece of oak. Accordingly, on-site finishing of the Staircase will result in
variations in colour, sheen and consistency of finish and, as such, the Staircase and the
hardwood flooring will differ in appearance.
12. Hardwood floors: Purchaser(s) are advised that the normal installation practice,
as recommended by the hardwood manufacturer, is to install the hardwood
perpendicular to the floor joists. Since not all floor joists run in the same direction
throughout the home, the Purchaser(s) acknowledge and accept that the hardwood will
not all run in one direction but will be installed as per the hardwood manufacturer’s
recommendation. The Purchaser accepts this method of installation.
13. Where hardwood floors are being installed as a standard feature or selected as an extra  by the Purchaser(s), in “wet” areas, including but not limited to the kitchen, breakfast, foyer, mudroom, etc, the Purchaser hereby releases the Vendor from all liability as it relates to water damage, swelling and/or imperfections that may exist as a result of the hardwood being installed in the wet areas.
14. All natural stone samples shown at the Décor Centre/Sales Office may vary from the
product received from the manufacturer for installation. Purchaser acknowledges and
accepts that the manufacturing process can result in differences in finish, colour, texture,
veining and after decorative attributes of the natural stone product. The Vendor does not
warrant the consistency of these attributes and reserves the sole and absolute discretion
to install the natural stone product. The Vendor reserves the right to install all tiles as
delivered in the pattern and location selection as decided with the sole discretion of the
Vendor’s installers and Purchaser irrevocably consents and agree to same.
15. Lighting: Purchaser(s) acknowledge and accept that due to construction and installation of framing members (lumber), plumbing pipes and HVAC systems, the location of ceiling electrical rough-ins and/or light fixtures and/or smoke and CO detectors may not be ‘centred’ within the ceiling space of any particular room(s).
16. Eco-laminate flooring may react to normal fluctuations of humidity levels by producing gapping or cupping, both of which shall be considered acceptable. The Purchaser acknowledges that failure to maintain a standard humidity level in the home may result in excessive gapping or cupping, for which the Vendor shall not be responsible.
17. Ceiling heights will be less than the stated ceiling height where ceiling bulkheads are
installed and where dropped ceilings are required.
18. If the home is at a stage of construction which will enable the Vendor to permit the
Purchaser to make colour and material choices from the Vendor’s standard samples,
then the Purchaser shall have until the date designated by the Vendor to properly
complete the Vendor’s colour and material selection form.
19. The Purchaser acknowledges that there shall be no reduction in the price or credit for
any standard feature listed herein which is omitted at the Purchaser’s request.
20. References to model types or model numbers refer to current manufacturer’s models
or Vendor’s house model, as the case may be. If these types or models shall change, the
Vendor shall provide an equivalent model (not applicable to Vendor’s house model).
21. Wall locations are approximate, and walls or portions of walls may be furred out, or have a vertical box installed altered to accommodate structural and/or mechanical requirements.
22. All measurement, specifications, sizes, products, materials and finishing details are
approximate, subject to change without notice and shall be from Vendor’s standard
samples, as applicable and as the circumstances may be.
23. Pursuant to this Agreement or this Schedule or pursuant to a supplementary
agreement or purchase order the Purchaser may have requested the Vendor to construct
an additional feature within the home which is in the nature of an optional extra
(such as, by way of example only, a fireplace); if, as a result of building, construction or
site conditions within the home or development, the Vendor is not able to construct
such extra, then the Vendor may, by written notice to the Purchaser, terminate the
Vendor’s obligation to construct the extra. In such event, the Vendor shall refund to
the Purchaser the monies, if any, paid by the Purchaser to the Vendor in respect of such
extra, without interest and in all other respects this Agreement shall continue in full
force and effect and the Vendor shall have no further obligation or responsibility to the
Purchaser, whatsoever, in respect thereof.
